**AMENDMENT 1**

**REQUEST FOR PROPOSALS**

**For**

**Warner Robins Middle School (WRMS) Track Repaving**

**RFP NUMBER 25-029**

**APPENDIX 1**

**Warner Robins Middle School Paving Requirements**

**PAVING REQUIREMENTS**

**RFP # 25-029**

**Warner Robins Middle School**

**425 Mary Lane**

**Warner Robins, GA 31088**

Add:

5. Grade and install a high jump pad and long jump runway and pit per NFHS standard sizes, dimensions, approach slopes and regulations. Each will be constructed on opposite ends of the field between the field goals and track.  Each asphalt section should consist of 6” GABC compacted to 95%  and 2” asphalt. The long jump runway shall be at least 130 feet long by 4 feet wide. The long jump pit shall have a minimum width of 9 feet and length of 23 feet and sand depth of 12”.  The pit shall have a 4 inch concrete curb. The take-off board must be at the same level as the top of the pit. All disturbed areas around each shall be graded and sodded with Tiff 419 Bermuda. The high jump should be 100 foot wide with a radius of 45 feet.