Specification for CNC Router

Turnkey MF 4X8 Router Special package-Forest Scientific CNC or equivalent equipment:

50" X 100" X 8.5" usable work area. To include:

Turnkey MF 4X8 Router special package

Includes vacuum table system with T slots and with 11.5 HP vac pump

5 HP HSD spindle

20 piece ER32 Collet set 1/16, 1/8 , 3/16, 7/32, (5)¼”, 5/16”, ⅜”, 7/16”, (4) ½”,9/16”, ⅝”, 11/16” ¾”

12 piece carbide starter tooling set (2) ¼” down, 2 (½”), (2) 60/90, (2) 10 deg, (2) ¼” ball, (1) 90 deg x ½” 49-SE1503, (1) 60 deg x ½” 49-SE1560

Control computer on support arm

Aspire software 40-seat educational license

Curriculum tutorials and videos

Automatic Z touch plate

3-year or greater on-site parts and labor warranty

Inside delivery, installation and on-site training

Dust hood

2 HP dust collector

Total bid for system, delivery, installation, and training: $\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Submitted by \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Company Name

Phone # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signature & Title of Company Official \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\*Contact WCTC Director Dr. Lisa Thompson for questions.

(931-722-5495