23-019 RE-KEYING SYSEMT

QUESTION & ANSWERS

1. The specs are showing to use Schlage Everest 29 key system. Does it need to be open or restricted T keyway cylinders/cores? Section 2.0.1.a – T is required it is the restricted key way.
2. Are interchangeable cores SFIC or FSIC? Section 2.0.1.b - FSIC
3. Do the rim, mortise, classroom, and non-classroom parts need to be conventional cylinders or removable cores? Section 2.0.1.b & 23-019 Response Form – It is both based on response form columns.
4. Is the rim, mortise, classroom, & non-classroom quantities for new locking hardware or just cylinder/cores only? i.e. does it require new ND series locks or the ND Classroom intruder conversion kit (40-301)? Section 2.0.1.a & 23-019 Response Form. - All Classroom must be intruder function conventional core, can use conversion kit or new hardware. All over doors will be cylinder replacement.
5. What does hardware change on 23-019 Response Form Mean? Section 2.0.1.a and 23-019 Response Form: - These are not Schlage will need to be replaced fully.
6. **Could you please clarify the following section 1.1 as it does not align with the attached document of materials and/or quantities listed per School. Must be Schlage Everest 29 cylinders**
7. **Could you please clarify the following section 2.0.1 as it does not align with section 1.1 or the attached document of materials and/or quantities listed per School.**

**Must be conventional and interchangeable core system currently in use in facilities. We have both in our system.**